Author: Kerron Martin

the

group

technology that works

“Evolution” E B45R-Sn
Revolutionising Refrigeration Today

All Purpose Display & Storage Refrigerator

Brilliant LED Sign Panel

Full height Internal LED “Twin” spread lighting

Automated and Manual Lighting control

Dual magnet door sealing and plastic fascia, thermal break

Ducted air flow system for even temperature distribution

Outstanding Energy Efficiency

Self closing toughened safety glass doors, double low E , Argon filled, incorporating the latest warm edge technology

Full Length Easy Grip Door Handle

EMS controller using “ smart memory functions” automatically saving you energy.

Easy access condenser Filter

Easy roll lockable castors

Door sensor controlled fan

“Shhhh” whisper quiet operation utilising patented EBM Evap and Condenser fan motors adding, efficiency and unparalleled reliability to the new Evolution models.

High Energy Efficiency

Evolution is an Easy Clip fully removable, universal, refrigeration package (one package fits all models).

Proudly Australian Designed
by The Orford Group
IP protected by AUS DSN no 345317

With Evolution comes much responsibility. The Orford Group continues to develop World Class Energy reduction systems to improve the lives of our customers and future generations.

1300 ORFORD (1300 673 673) +617 4641 7372
sales@theorfordgroup.com.au www.theorfordgroup.com.au

PO Box 18120 Clifford Gardens Queensland 4350 Australia

January 2013 Ver 1.

The Orford Group reserves the right to alter specifications without notice.

The Orford Group reserves the right to alter specifications without notice.

October 2012 Ver 1.

October 2012 Ver 1.

the

“Evolution” E B45R-Sn
Three Door Vertical Display Refrigerator

group

Features
World class,
> Design
> Energy Efficiency
> Performance
> Quality
> Reliability
Universal Refrigeration Package
> One package fits the entire E B Range
> Cassette Style: Removable without tools
> Minimal training required for
non-qualified personal to replace the package

Energy Management System (EMS)
> Automatically learns you trading times
> Automates your energy savings
> Perishable and non-perishable mode
Lighting Control
> Automated or manual control, you choose
> Independent switching of interior and sign lighting
Condenser Fan Function
> Your choice of reversing or non-reversing function
Condenser Filter
> Easy Access filter: No tools, no covers to remove

E

E

E

E

E

E

High Energy Efficiency

E B45R-Sn / Specifications	Vertical Display Refrigerator with Illuminated Advertising Sign
Construction	Powder Coated galvanized steel Interior / Exterior White
Capacity	1384 Litres (Gross)
Dimensions	1460W x 762D x 2220H
Weight	265 Kg
Operating Temp	0° - 5° C.
Ambient Temp Range	0° - 40° C.
Power Point	220 - 240v 50Hz. (Standard GPO)
Input Current	3.2 Amps
Thermometer	Digital
Shelves	12 Height Adjustable Heavy Duty PVC Coated
Shelves	3 Fixed Stainless Steel Base Shelves
Shelf Adjustment	12mm Increments
Refrigerated Shelf Area	3.38 m²
Condensate Disposal	Automatic by energy efficient, No Cost, Hot Gas
Door	3 x Self Closing, Double Glazed Safety Glass, Double Heat reflective Low E, Warm edge
Footings	Heavy Duty Castors, Lockable Front
Interior Light	LED, Automatic and manual control
Refrigerant	R134a
Drier	Solid Core
Insulation	50mm Polyurethane, CFC, HCFC, HFC Free
Cabinet Classes	3M1, 4M1, 5M1
MEPS	Compliant (High Efficiency)
* Energy Consumption	6.03 kWh/24h
Condenser Filter	Easy front access
Illuminated Advertising Sign	200mm High, Top Mounted
Sign Illumination	LED, Automatic and manual control

* Energy Consumption measured at 25°C. Cabinet Class 3M1 as per Australian Standard AS1731

IP protected by AUS DSN no 345317

+617 46345 278 +617 4641 7372
sales@theorfordgroup.com.au www.theorfordgroup.com.au

PO Box 18120 Clifford Gardens Queensland 4350 Australia

January 2013 Ver 1.